z (m): depth below the ground surface to the tip of the cone penetrometer
qc (MPa): cone tip resistance
fs (kPa): sleeve friction
u2 (kPa): pore pressure behind cone
location: (x,y) coordinates (in meter) for all soundings